
Assignment 5 Arduino Application

**Task** Design a circuit using a temperature sensor, three LEDs indicate different levels of temperature stages, the detailed information will be displayed on LCD1602. Once the simulated temperature is over the 60 degrees Celsius, then the piezo will give an alarm to indicate overheating.

Answer:



#include <LiquidCrystal.h>  
LiquidCrystal lcd(13, 12, 7, 6, 5, 4);  
int baselineTemp=0;  
int celsius=0;  
int fahremheit=0;  
unsigned long tepTimer ;  
String ledColor[3]={"red","Greed","blue"};  
  
void setup(){  
  Serial.begin(9600);  
  pinMode(3,OUTPUT);  
  pinMode(8,OUTPUT);  
  pinMode(9,OUTPUT);  
  pinMode(10,OUTPUT);  
  lcd.begin(16,2);  
  lcd.setCursor(0,0);  
  lcd.print("Current Temp is:");  
}  
  
void loop(){  
  celsius = map(((analogRead(A0)-20)\*3.04), 0, 1023, -40, 125);  
  fahremheit = ((celsius \* 9)/5 + 32);  
    lcd.setCursor(0,1);  
    lcd.print(celsius);  
    lcd.setCursor(4,1);  
    lcd.print("Degree");  
    
    Serial.print(celsius);  
    Serial.print(" C, ");   
    Serial.print(fahremheit);  
    Serial.println(" F");  
  
    if(celsius<50){  
      lcd.setCursor(0,0);  
      lcd.print("Current Temp is:");  
      digitalWrite(8,HIGH);  
      digitalWrite(9,LOW);  
      digitalWrite(10,LOW);  
      digitalWrite(3,LOW);  
  
    }  
    if(celsius>=50&&celsius<60){  
      lcd.setCursor(0,0);  
      lcd.print("Current Temp is:");  
      digitalWrite(8,HIGH);  
      digitalWrite(9,HIGH);  
      digitalWrite(10,LOW);  
      digitalWrite(3,LOW);  
  
    }  
    if(celsius>=60){  
      lcd.setCursor(0,0);  
      lcd.print("Current Temp is:");  
      digitalWrite(8,HIGH);  
      digitalWrite(9,HIGH);  
      digitalWrite(10,HIGH);  
      digitalWrite(3,HIGH);  
    
    }  
}